**EXPERIMENT 5**

TO DETERMINE THE CRITICAL LOAD AND BUCKLING IN LONG COLUMNS





