Name TAHIR ULLAH

ID NO 14033

PAPER BIOMEDICAL LAB

INSTRUMENTATION

INSTRUCTOR MS SAIMA HADI

BS MLT 6TH

**Q1. DEFINE THE FOLLOWING**

1. **PH METER,**

PH mean power of hydrogen or to measure the H ion activity in water based solutions (acidity) or alkalinity.

It is an electric device which is used to find out the acidity and basicity or alkalinity of a solution.

It was discovered by American chemist named Arnold, through which we want to measure the sourness of lemons.

1. **VORTEX MIXER,**

it is also known as vortexer….

It is simple device dedvice of equipment mostly found in different research labs and it is used to mixed the small particles or samples of liquid solution.

This device can also do single test and multiple liquid samples at a time.

1. **BALANCE,**

It is a weighting scale is a device which is used to measureing weights.

It measures the mass of an object and also used in different fields such as

1. **WATER STILL,**

It is a water heating device in which wateris heated until change into steam. Then collected that steam in tubes or glasses and then finally condense that steam into new purified water droplets and then collected in a new clean vessel.

1. **DEIONIZED,**

As the name indicate that it is a process in which the ions are remove from the water solution ions including minerals, salts, iron, sodium etc

**Q2. ELECTROPHORESIS**

Electrophoresis is a laboratory technique used to separate DNA, RNA, or protein molecules based on their size and electrical charge. An electric current is used to move molecules to be separated through a gel. Pores in the gel work like a sieve, allowing smaller molecules to move faster than larger molecules. The conditions used during electrophoresis can be adjusted to separate molecules in a desired size range.

Electrophoresis is a very broadly used technique which, fundamentally, applies electric current to biological molecules, whether--they're usually DNA, they can be protein or RNA, too...and separates these fragments into pieces which are larger or smaller. It's used in a variety of applications... Everything from forensics for determining the identity of individuals that may have been involved in a crime, by linking their DNA pattern,

**IMPORTANCE OF ELECTROPHORESIS**

1. It is used in DNA fingerprinting.
2. It is also used inpaternity testing.
3. In forensic study (crimionology)
4. Very useful in genetic and in study of molecular biology.
5. Commonly used in DNA sequencing.
6. Purification and analyzing of vaccine.

**Q 3. FLOW CYTOMETERY,**

It is a technique which is used to detect or analyze the physical and chemical properties or characteristics of different due to excitments.

Hundreds to thousand of particles are analyze as they passed through liquid steam.

**PRINCIPLE**

**The** flow system (fluid); cell in suspension are bought in a single file past.

THE OPTICAL SYSTEM (light sensing); a focused laser which scatter light and emits fluorescence that is filtered and collected.

THE ELECTRICAL SYSTEM (signal processing): Emitted light is converted to digitized of values that are stored in a file for analysis.

**APPLICATIONS:**

* Immunophenotyping of lymphoma and leukemia
* Detection of malignancy in body fluids
* DNA ploudy and cell cycle analysis.
* CD4 and CD8 counting.
* Histocompatibility cross matching .
* Reticulocytes count.
* PNH detection
* HLA-B27 detection
* Bioterrorism
* Parasitology
* Microbiology
* Molecular biology
* Genetics
* Cell kinetics
* Immunofluorescence
* Cell cycle kinetics
* Animal husbandry
* Biological oceanography
* Minimal residual disease
* Apoptosis and gene reporter

**Q4. What do you know about beer lambert law (uses, principle)?**

**Answer no question 4**

**Beer lambert law:**

* Beer –lambert law state that the quantity of light absorbed by a substance dissolved in transmitting solvent directly proportional to the concentration of the substance and the path length of the light through the solution.

**Uses of beer-lambert low:**

* Its used for detection of bilirubin in blood sample
* Uses for the analysis of mixture of substance by spectrophotometry
* Use for measure of absorbance of unknown sample.
* Use for the measurement of absorbance of standard solution
* It use for the detection of iron in industrial steam.

**Principle**

* UV –visible spectroscopy measure the response of a sample to ultra violet and visible range of electromagnetic radiation
* Molecule have either n,π,Ჾ, electron .theses absorbed UV radiation and undergoes transition from ground state to excited state.
* the autoclaved in the laboratory the most agreeable and commonly used method is to use steam at 121oC for 15 to 30 minutes depending upon the particular material to be sterilized .

**Q5. AUTOCLAVE,**

The Autoclave carries out that exact function of sterilizing materials. It is a machine that uses pressure and steam to reach and maintain a temperature that is too high for any microorganisms or their spores to live.

Microorganisms are what most people commonly refer to as germs.

**USES OF AUTOCLAVE,**

A medical autoclave is a device that uses steam to sterilize equipment and other objects.this means that all bacteria, viruses, fungi and spore are inactivated….

Autoclave are found in many medical setting, laboratories and other places that need to ensure the sterility of an object.

**CRITICAL COMPONENT OF AN AUTOCLAVE**

Chamber, the chamber is the primary component of a steam autoclave, consisting of an inner chamber and outer jacket….

* Controls system….
* Thermostatic trap..
* Safety valve…
* Waste-water cooling mechanism…
* Vacuum system (if applicable)
* Steam generator (if applicable).