**What is difference between Circuit switching and Packet switching. Answer should not be more than four to five lines.**

**One of the disadvantages of using point to point (Mesh) network is that the number of connections grows more rapidly as the number of computers increase. Find the number of connections needed to be used in point to point (Mesh) topology in network of 10 and also find that how many I/O ports are needed for each device.**